ANSI PUBLIC REVIEW

Public Comment Form

BSR B109.5 Standard: Self-Operated Diaphragm-Type Natural Gas Service Regulators

for nominal pipe size up to and including 2 inches (50 mm) and inlet pressures up to 125 psig (861.6 kPa)

**Return this completed form to B109 Committee Secretary Luis Escobar at** [**lescobar@aga.org**](mailto:lescobar@aga.org) **by 2 October 2023.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Your Name:** | **Your Company:** | **Your Email:** | **Your Phone:** |

| **Name:** | **Company:** | **Chapter, page, section:** | **Comment / Suggested Changes**  **(Copy from the text the relevant sentence(s), paste here and track change with proposed language)** | **Reason** |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |